C4BH2WF1 - 206 CABRIOLET

REMOVAL - REFITTING SCREEN (LUGGAGE COVER) SWITCH

1 - REMOVAL

Change the vehicle into the coupé version .

Open the luggage compartment .

Fold up the tray (luggage cover screen) .

Disconnect the connector(1) via the lights access cut-out in the left side trim (2) .

Remove :

- the securing bolt (3)
- the screen switch assembly with its support (4) by unclipping it upwards (A)

2 - REFITTING

Proceed in the reverse order to removal .

Test operation .