C5GG2BF1 - 206 CABRIOLET

REMOVAL - REFITTING REAR QUARTER PANEL SIDE TRIM PANEL

Place the vehicle in cabriolet position .

1 - REMOVAL

Remove :

- THE REAR QUARTER PANEL SIDE TOP TRIM
- THE REAR SEAT
- THE REAR SEAT BACK REST

Dislodge the door opening seal (1) .

Remove the rear seat belt lower fixing (2) .

Remove the clip (3) .

Unclip the side trim (4) on both sides and at the top from the passenger compartment partition trim (5) at (A) .

Unclip and remove the rear quarter panel (4) panel .

2 - REFITTING

Proceed in the reverse order to removal .

Fit :

- THE REAR SEAT BACK REST
- THE REAR SEAT
- THE REAR QUARTER PANEL SIDE TOP TRIM

Seat belt fixing tightening torque 3 ± 1 da.Nm .