C4BG18F1 - 206 CABRIOLET

REMOVAL - REFITTING MOVING REAR SHELF HINGE MECHANISM

1 - REMOVAL

Remove :

- THE MOVING REAR SHELF
- THE DETACHABLE REAR SHELF STRUT (without disconnecting the pipes)

Remove the 4 bolts (1) (On both sides) .

Unclip the harness clamp (2) .

Disconnect the electrical connections (3) - (4) .

Remove the hingeing mechanism of the mobile rear shelf (5) .

2 - REFITTING

Proceed in the reverse order to removal .

Test operation .