C5FG1PF1 - 206

REMOVAL - REFITTING FLOOR CONSOLE

1 - REMOVAL

Remove the fastener (1) .

Pull the storage compartment towards the rear to detach it .

Remove :

- the storage compartment

Remove the fasteners (2) .

Detach the handbrake lever .

Using a spatula, Unclip :

- the gear lever gaiter assembly (3)
- the cover (4)
- the coin storage compartment (6)
- the fasteners (5)

Remove the fastener (7) .

Lift the console and disconnect the connectors (according to specification) .

Raise the console from the rear .

Pull the console towards the rear to detach the front section from the fascia .

Remove the console .

2 - REFITTING

Proceed in the reverse order to removal .